НАЦІОНАЛЬНИЙ ТЕХНІЧНИЙ УНІВЕРСИТЕТ УКРАЇНИ

«КИЇВСЬКИЙ ПОЛІТЕХНІЧНИЙ ІНСТИТУТ ІМЕНІ ІГОРЯ СІКОРСЬКОГО»

Кафедра автоматизації проектування енергетичних процесів і систем

Тема 8. Завдання 1

З дисципліни: «Розробка стартап-проектів»

**Виконав:**

студент 5 курсу

групи ТР-02мп, ТЕФ

Круглий Д.В.

**Перевірила:**

доц. Копішинська К.О.

Київ – 2021

**Патентний пошук**

***Команда:*** Круглий Д.В. (гр. ТР-02мп), Орихівський Є.Р. (гр. ТР-01мп).

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **№ з/п** | **Країна патентування** | **Шифр документа** | **П.І.Б. автора ідеї** | **Назва документу і стислий опис ідеї** |
| 1 | US | 10440545 | Horton, David (San Jose, CA, US)  Tan, Leon (San Jose, CA, US)  Urman, Andrew (San Jose, CA, US)  Daniels, Melissa (San Jose, CA, US) | Systems and Methods disclosed herein relate to providing control of smart devices via data provided from or to a doorbell, via an application programming interface (API). |
| 2 | Taiwan | 9965967 | Lee, Yu-tzu (Changhua, TW)  Chen, Tsair-rong (Changhua, TW) | An RFID book detection system for school children may comprise a plurality of book jackets, at least an assignment system, and a school bag. The book jackets respectively fit around different books, and each of the book jackets has a corresponding RFID tag on a surface thereof. |
| 3 | US | 9965819 | Devries, John (Palm Desert, CA, US) | School District Administrators have the real-time monitoring of students and school buses during daily school transportation. The IRITRANS® system will provide school districts with real-time bus locations and more importantly the “specific identity of all students on-board”. |
| 4 | US | 8108307 | Kawan, Joseph C. (Hollywood, CA, US)  Munoz, Ramiro (Santa Monica, CA, US)  Kogen, Mark (Lawndale, CA, US) | A system, method and apparatus for exchanging value using a smart card in a financial transaction is disclosed. The system includes a smart card having a contact interface and a contactless interface interactive with a closed purse application and an open purse application controlled by a microprocessor. |